|  |
| --- |
| **FTM® Symons Cone Crusher Model Specifications**  email: customer@sinoftm.com |
| Type | Model | Diameter of large end of crushing cone(mm) | Adjusting Range of Discharge Opening(mm) | Feed opening size of the open edge when recommending the min. Discharge opening(mm) | Max.feeding size(mm) | Processing capacity(t/h) | Main motor power(kw) | Machine weight(kg) |
| PSG 900 | 0910 | 914 (3′) | 9-22 | 102 | 85 | 45-91 | 6P   75 | 9980 |
| 0917 | 13-38 | 175 | 150 | 59-163 |
| 0904 | 3-13 | 41 | 35 | 27-90 |
| 0906 | 3-16 | 76 | 65 | 27-100 |
| PSG 1300 | 1313 | 1295 (4¼′) | 13-31 | 137 | 115 | 109-181 | 6P   160 | 22460 |
| 1321 | 16-38 | 210 | 178 | 132-253 |
| 1324 | 19-51 | 241 | 205 | 172-349 |
| 1306 | 3-16 | 64 | 54 | 36-163 |
| 1308 | 6-16 | 89 | 76 | 82-163 |
| 1310 | 8-25 | 105 | 89 | 109-227 |
| PSG 1600 | 1620 | 1676 (5½′) | 16-38 | 209 | 178 | 181-327 | 6P   250 | 43270 |
| 1624 | 22-51 | 241 | 205 | 258-417 |
| 1626 | 25-64 | 269 | 228 | 299-635 |
| 1607 | 5-13 | 70 | 60 | 90-209 |
| 1608 | 6-19 | 89 | 76 | 136-281 |
| 1613 | 10-25 | 133 | 113 | 190-336 |
| PSG 2100 | 2127 | 2134 (7′) | 19-38 | 278 | 236 | 544-1034 | 6P   400 | 86730 |
| 2133 | 25-51 | 334 | 284 | 862-1424 |
| 2136 | 31-64 | 369 | 314 | 1125-1814 |
| 2110 | 5-16 | 105 | 89 | 218-463 |
| 2113 | 10-19 | 133 | 113 | 404-580 |
| 2117 | 13-25 | 178 | 151 | 517-680 |

Symons cone crusher

Email: customer@sinoftm.com

Website: http://www.miningftm.com/products/crushing/cone-crushers/symons-cone-crusher/